View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What actions can I configure if I press and hold the trigger button for 3 seconds?

In Single, Burst, or Self trigger modes you can set how the reader should react to pressing the button for 3 seconds. If you check more options, the functionality runs in the listed order.

Pressing and holding the trigger button on the reader for 3 seconds can:

- Optimize the brightness in your acquired images, if these operations are supported by the current trigger mode

- Read a Configuration Code from the Configuration Codes document

- Train the reader with the symbology you expect in successive symbols

- Set a match string if you are performing match string validation

- Put the device into Test Mode

Pressing and holding the trigger button is the same as using the trigger button on the button bar of the Setup Tool.

Note: DM503