View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is Motion Detection?

Motion Detection allows you to set up your device to switch into active Presentation or Self trigger mode for a period of time after it detects movement in the device's field of view.

Motion Detection settings become available only if the trigger type is set to Presentation or Self. When Motion Detection is enabled, the device is not taking images, but monitors the background if the scene in its field of view is in motion or not.

If it is in motion, the device actively acquires images as per Presentation or Self trigger mode. The Timeout setting allows you to specify the time period (in seconds) after which the device switches back to Motion Detection from active triggering, but this Timeout resets every time by motion or a good read.

With Motion Detection Sensitivity you can define the device's sensitivity to recognize motion. For example, if it is set to High, the device switches on active Presentation and Self trigger modes even if the amount of motion in the field of view was small.

Note: DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503