View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Which Non-Printing Characters are converted?

Eight-bit ASCII character codes with values of 0x00 through 0x1F and 0x7F are converted when Translate Unprintable Characters is enabled. The characters are mapped to a the ASCII character name, as listed here:

0x00 <NUL>

0x01 <SOH>

0x02 <STX>

0x03 <ETX>

0x04 <EOT>

0x05 <ENQ>

0x06 <ACK>

0x07 <BEL>

0x08 <BS>

0x09 <HT>

0x0A <LF>

0x0B <VT>

0x0C <FF>

0x0D <CR>

0x0E <SO>

0x0F <SI>

0x10 <DLE>

0x11 <DC1>

0x12 <DC2>

0x13 <DC3>

0x14 <DC4>

0x15 <NAK>

0x16 <SYN>

0x17 <ETB>

0x18 <CAN>

0x19 <EM>

0x1A <SUB>

0x1B <ESC>

0x1C <FS>

0x1D <GS>

0x1E <RS>

0x1F <US>

0x7F <DEL>

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503