View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How do I use the Update Firmware function?

This function updates the selected device or devices to the desired firmware version.

1. Select the device or devices you want to update from the device list.

2. Browse for firmware files by clicking the '...' icon. If a single device is selected in the device list, the appropriate firmware folder for that device is opened. If multiple devices are selected, but they have the same firmware device ID, the appropriate folder is opened. If no device is selected or more devices are selected, but they have different firmware device IDs, the root firmware folder is opened.

3. Click the Upload Firmware button. The button is enabled only if the selected firmware version and device selection is compatible.

4. In the window that pops up, check Backup device before firmware update if you want the Setup Tool to back up configuration files the same way the Backup function does (see Backup Q and A for more details).

5. Click Yes to start uploading the new firmware.

Note: In case of serial devices, you need to discover them first by manually refreshing before being able to update firmware.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503,DM7500,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500,RTM_Lean