View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can the "Always on" Enabled option in the High Frequency Lights box be used for?

If internal illumination is turned off, and therefore High Frequency Lights are enabled, you can set here a timeout after which the High Frequency Light (HFL) is turned off if no trigger occurred for a long period of time. The timeout is specified in seconds. Setting the timeout value to 0 turns off the timeout handler and the light will stay on forever. Changing operation mode or turning the live image view on will turn off the HFL.

Note: DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503