# IMAGEBUFFER.RECORD-TYPE

Sets or gets the type of image to buffer.

Note: In case of No-Read, the image is buffered if the reader fails to read.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type | enum | [0-5] | 0: None 1: No-Read 2: Read 3: All 4: Validation Failure 5: No-Read + Validation failure

## Platforms

DM50, DM60, DM70, DM300, DM360, DM370, DM470, DM8000, DM503, MX-1000

## Notes

Version: 4.0.0