# COM.XLATEPRNT

Translate unprintable characters that are embedded in a symbol. The translated result is output over the connection (for example, COM, USB, Ethernet, USB-KEYBOARD). Note that Data Formatting leading and terminating text are not translated. The characters translated are ASCII values between 0x00 and 0x1F. For example, 0x00 = <NUL>, 0x04 = <EOT>, 0x0a = <LF>, 0x0d = <CR>.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | enable/disable

## Platforms

ALL

## Notes

Version: 3.0.0