# Communication Overview

Command | Supported Platforms
--- | ---
ACCEL-SENSOR.OPERATION-MODE | DM8050, DM8600.
ACCEL-SENSOR.SENSITIVITY | DM8050, DM8600.
ANDROID.AOA-SWITCH-TIMEOUT | MX-1000, MX-1502
ANDROID.ROLE | MX-1000, MX-1502
BLUETOOTH.HID-RECONNECT | DM8700
BLUETOOTH.MAC-ADDRESS | DM8050, DM8600.
BLUETOOTH.MAX-RF-POWER | DM8050, DM8600, and Bluetooth base stations.
BUTTON.SAVE-MATCH-STRING | DM80, DM280, DM300, DM360, DM370, DM470, DM503
COM.BAUD-RATE | ALL except for MX-1000.
COM.BUFFER-AUTO-FLUSH | Wireless readers.
COM.BUFFER-DATA | Wireless readers.
COM.BUFFER-MODE | Wireless DM8000 readers.
COM.COMMUNICATIONS-MODULE | MX-1000 and DM8000.
COM.DATA-BITS | ALL except for MX-1000.
COM.DMCC-DEFAULT-TARGET | DM8700 Base
COM.DMCC-RESPONSE | ALL
COM.DMCC-TARGET | DM8700 Base
COM.MULTI-PORT | DM50, DM60, DM70, DM150, DM260, DM300, DM370, DM470, DM475V, DM503
COM.PARITY | All except for MX-1000 and MX-1502.
COM.PROTOCOL | Devices with RTS/CTS lines
COM.READER-IN-CRADLE | DM8700, DM8700 base station
COM.RS232-ENABLE-PAUSE | DM80-USB, DM280, DM300, DM360, DM370, DM470, DM60, DM50, DM70.
COM.RS232-INTERCHAR-DELAY | DM80-USB, DM280, DM300, DM360, DM370, DM470, DM60, DM50, DM70, DM503.
COM.RS232-ROUTE | DM80-USB, DM280, DM8000 wireless readers.
COM.SCRIPT | Fixed-mount readers
COM.SCRIPT-ENABLED | Fixed-mount readers
COM.SCRIPT-ERROR | Fixed-mount readers
COM.STOP-BITS | ALL except for MX-1000.
COM.USB-COMPATIBILITY-MODE | DM50, DM70, DM80-USB, DM280, DM8000
COM.USB-DROP-WITHOUT-DTR | DM80-USB, DM280, DM8700
COM.USB-HID-ENABLE | DM80-USB, DM280, DM8700 base station USB, DM8700 USB
COM.USB-HID-IGNORE-CAPS-LOCK | DM80-USB, DM280, DM8700 base station USB, DM8700 USB
COM.USB-HID-NO-OUT-ENDPOINT | DM80-USB, DM280, DM8700 base station USB, DM8700 wired USB
COM.USB-HID-ONLY | DM80-USB, DM280, DM8000 base station G2, DM8700 base station USB, DM8700 wired USB
COM.USB-MODE | DM50, DM60, DM70, DM80-USB, DM280, MX-1000, MX-1502 and DM8000.
COM.USB-RE-ENUMERATE-ON-START | DM80-USB, DM280, DM8000.
COM.USB-REQUIRE-DTR | DM80-USB, DM280, DM8050, DM8700
COM.USB-REQUIRE-DTR | DM50, DM60, DM80-USB, DM150, DM280
COM.USB-SERIAL-COM | DM80-USB, DM280
COM.USB-SPEED | Every reader connected through USB except MX-1000 and DM80-PoE.
COM.WAKEUP | ALL
COM.XLATEPRNT | ALL
CONFIG-BACKUP.SERVER-TYPE | DM300, DM360, DM370, DM470, DM503
CUSTOM-CMD.COMMAND-FOOTER | Fixed mount readers.
CUSTOM-CMD.COMMAND-HEADER | Fixed mount readers.
CUSTOM-CMD.ECHO | Fixed mount readers.
CUSTOM-CMD.TRIGGER | Fixed mount readers.
CUSTOM-CMD.TRIGGER-OFF | Fixed mount readers.
CUSTOM-CMD.TRIGGER-ON | Fixed mount readers.
DATA.RESULT-ENCODING | ALL
DEVICE.MAC-ADDRESS | Ethernet readers.
DEVICE.SSID | Wireless readers.
ETHERNET-IP.ENABLED | Ethernet readers. The DM8000 wireless readers also support this protocol if the base station is connected through Ethernet. In the case of a Bluetooth connection, the command has to be sent to the base station, not to the reader.
FTP-IMAGE.CUSTOM-FILE-NAME | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-IMAGE.FILE-NAME | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-IMAGE.FILE-NAME-USE-SCRIPT | DM80, DM280, DM300, DM360, DM370, DM470, DM503
FTP-IMAGE.IDLE-LIMIT | DM80, DM280, DM300, DM360, DM370, DM470, DM503
FTP-IMAGE.IDLE-TIME | DM80, DM280, DM300, DM360, DM370, DM470, DM503
FTP-IMAGE.IP-ADDRESS | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-IMAGE.MAX-APPEND | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-IMAGE.MAX-APPEND-START-VALUE | DM503
FTP-IMAGE.PASSWORD | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-IMAGE.PORT | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-IMAGE.SERVER-PATH | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-IMAGE.SERVER-PATH-SCRIPT | DM80, DM280, DM300, DM360, DM370, DM470, DM503
FTP-IMAGE.SERVER-PATH-SCRIPT-ERROR | Fixed-mount readers
FTP-IMAGE.SERVER-TYPE | DM80, DM280, DM300, DM360, DM370, DM470, DM503
FTP-IMAGE.USER-NAME | Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-PCM-REPORT.CUSTOM-FILE-NAME | PCM-enabled readers
FTP-PCM-REPORT.ENABLE | PCM-enabled readers
FTP-PCM-REPORT.FILE-NAME | PCM-enabled readers
FTP-PCM-REPORT.FILE-NAME-USE-SCRIPT | PCM-enabled readers
FTP-PCM-REPORT.IDLE-LIMIT | PCM-enabled readers
FTP-PCM-REPORT.IDLE-TIME | PCM-enabled readers
FTP-PCM-REPORT.IP-ADDRESS | PCM-enabled readers
FTP-PCM-REPORT.MAX-APPEND | PCM-enabled readers
FTP-PCM-REPORT.MAX-APPEND-START-VALUE | PCM-enabled readers
FTP-PCM-REPORT.PASSWORD | PCM-enabled readers
FTP-PCM-REPORT.PORT | PCM-enabled readers
FTP-PCM-REPORT.SCRIPT-ERROR | PCM-enabled readers
FTP-PCM-REPORT.SERVER-PATH | PCM-enabled readers
FTP-PCM-REPORT.SERVER-TYPE | PCM-enabled readers
FTP-PCM-REPORT.USER-NAME | PCM-enabled readers
FTP-RESULT.APPEND | Ethernet readers. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-RESULT.ENABLE | Ethernet readers. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-RESULT.FILE-NAME | Ethernet readers. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-RESULT.IDLE-LIMIT | DM80, DM280, DM300, DM360, DM370, DM470, DM503, DM8700 base stations, DM8700 Ethernet readers
FTP-RESULT.IDLE-TIME | DM80, DM280, DM300, DM360, DM370, DM470, DM503, DM8700 base stations, DM8700 Ethernet readers
FTP-RESULT.IP-ADDRESS | Ethernet readers and MX-1000. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-RESULT.PASSWORD | Ethernet readers. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-RESULT.PORT | Ethernet readers. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
FTP-RESULT.SERVER-TYPE | DM80, DM280, DM300, DM360, DM370, DM470, DM503, DM8700 base stations, DM8700 Ethernet readers
FTP-RESULT.USER-NAME | Ethernet readers. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.
HPIT.FRONT-COVER | DM370, DM470
INPUT1.SAVE-MATCH-STRING | DM50, DM60, DM70, DM280, DM300, DM360, DM370, DM470, DM503
INTER-MESSAGE.DELAY | Wireless readers.
KEY.BLUETOOTH-EJECT-BUTTON | DM8700 Bluetooth readers
KEY.CONTROL-CHARACTERS-MAPPING | DM8700 USB, DM8700 Base Station USB
KEY.INTERCHAR-DELAY | DM50, DM60, DM70, DM80-USB, DM280, DM300, DM360, DM370, DM470, DM8700 base station USB, DM8700 USB
KEY.REDUCE-KEY-UP-USAGE | DM80-USB, DM280, DM8700 base station USB, DM8700 USB
KEY.REPORT-INTERVAL | DM80-USB, DM280, DM8700 base station USB, DM8700 USB
KEY.SEND-PHYSICAL-CONTROL-CHARACTERS | DM8700 USB, DM8700 Base Station USB
MASTER-SLAVE.GROUP-NAME | DM60, DM80-PoE, DM280, DM300, DM360, DM370, DM470, DM503
MASTER-SLAVE.MODE | DM60, DM80-PoE, DM280, DM300, DM360, DM370, DM470, DM503
MASTER-SLAVE.TEST | Fixed-mount readers, except DM80-USB
MASTER-SLAVE.TEST-EFP-OUTPUT | DM80-PoE, DM280, DM300, DM360, DM370, DM470
MASTER-SLAVE.TIMEOUT | DM60, DM80-PoE, DM280, DM300, DM360, DM370, DM470, DM503
MASTER-SLAVE.TIMEOUT-DISTANCE | DM60, DM70, DM80-PoE, DM260, DM280, DM300, DM360, DM370, DM470, DM503
MASTER-SLAVE.TIMEOUT-MODE | DM60, DM80-PoE, DM260, DM280, DM300, DM360, DM370, DM470, DM503
MAXICODE.PERSPECTIVE-DISTORTION | DM280, DM370, DM470
MODBUSTCP.ENABLED | Ethernet readers. The DM8000 wireless readers also support this protocol if the base station is connected through Ethernet. In the case of a Bluetooth connection, the command has to be sent to the base station, not to the reader.
MODBUSTCP.HOLDING-ONLY | Ethernet readers. DM8000 wireless readers also support this protocol if the base station is connected through Ethernet.
NET-LOCAL.DHCP | Ethernet readers.
NET-LOCAL.DNS-SERVER | Ethernet readers.
NET-LOCAL.GATEWAY | Ethernet readers.
NET-LOCAL.IP-ADDRESS | Ethernet readers.
NET-LOCAL.PORT | Ethernet readers.
NET-LOCAL.READER-IP-ADDRESS | Base stations.
NET-LOCAL.READER-SUBNET-MASK | Base stationss.
NET-LOCAL.SUBNET-MASK | Ethernet readers.
NETWORK-CLIENT.CLIENT-PORT | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.CLOSE-CONNECTION | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.CONNECTION-TIMEOUT | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.ENABLED | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.HOST-ADDRESS | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.HOST-PORT | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.IDLE-TIMEOUT | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.OPEN-CONNECTION | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.PROTOCOL | Ethernet readers except for the DM8000 wireless.
NETWORK-CLIENT.RECONNECT-DELAY | Ethernet readers except for the DM8000 wireless.
NTP.ENABLE | All
NTP.SERVER1 | All
NTP.SERVER2 | All
OUTPUT.USER-CONFIGURE | DM80, DM280, DM8050, DM8600, MX1000.
PROFINET.ENABLED | Ethernet readers. The DM8000 wireless readers also support this protocol if the base station is connected through Ethernet. In the case of a Bluetooth connection, the command has to be sent to the base station, not to the reader.
PTP-SYNC.DELAY | DM80, DM280, DM370, DM470
PTP-SYNC.DELAY | DM360
PTP-SYNC.ENABLE | DM80-PoE, DM280, DM360, DM370, DM470
PTP-SYNC.LOCAL-OFFSET | DM80, DM280, DM360, DM370, DM470
PTP.ENABLE | DM80-PoE, DM280, DM360, DM370, DM470
PTP.SLAVE-ONLY | DM80-PoE, DM280, DM360, DM370, DM470
QR.PERSPECTIVE-DISTORTION | DM80, DM280, DM370, DM470
READER.ASSIGNED | Base
SDCARD.BACKUP-FILE | DM360, DM370, DM470
SDCARD.PRESENT | DM360, DM370, DM470
SET-WIRELESS.LINK-TIMEOUT | DM8700 Bluetooth reader
SLMP-PROTOCOL.ENABLED | Ethernet readers. DM8000 wireless readers also support this protocol if the base station is connected through Ethernet. In the case of a Bluetooth connection, the command has to be sent to the base station, not to the reader.
SYNC-ACQUISITION.CABLE-END | DM503
SYNC-ACQUISITION.DELAY | DM503
SYNC-ACQUISITION.ENABLED | DM503
SYNC-ACQUISITION.MASTER | DM503
TELNET.CUSTOM-PORTS | Ethernet readers
TELNET.PORT | Ethernet readers.
TEST-MODE.ACCEPT-TRIGGERS | DM70, DM150, DM260, DM300, DM360, DM370, DM470, DM503
TEST-MODE.AUTOMATIC | DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503
TEST-MODE.AUTOMATIC-OFF-US | DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503
TEST-MODE.AUTOMATIC-ON-US | DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503
TEST-MODE.ENABLE | DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503
TEST-MODE.INPUTS-ENABLE | DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503
TEST-MODE.OUTPUTS-ENABLE | DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503
WIFI.AP-BSSID | DM8700 Wi-Fi reader
WIFI.AP-CHANNEL | DM8700 Wi-Fi reader
WIFI.AP-SIGNAL | DM8700 Wi-Fi reader
WIFI.AUTH-MODE | DM8000
WIFI.BAND | DM8700 Wi-Fi reader
WIFI.CA-CERT | DM8000;Base
WIFI.CHANNEL |
WIFI.CLIENT-CERT | DM8000;Base
WIFI.CLIENT-IDENTITY | DM8000;Base
WIFI.CLIENT-PRIVATE-KEY | DM8000;Base
WIFI.ENABLED |
WIFI.ENC-METHOD | DM8000;Base
WIFI.NETWORK-TYPE | DM8000
WIFI.PASSPHRASE | DM8000;Base
WIFI.SCAN-CHANNELS | DM8700 Wi-Fi reader
WIFI.SSID |
WIFI.SUPPLICANT-LOG | DM8700 Wi-Fi reader
​MASTER-SLAVE.REFERENCE | ​Fixed-mount readers, except DM80-USB