# INPUT-STRING.ENABLE

Enables or disables the use of the Input String feature (available for serial, telnet, NetworkClient). When enabled, a header and the footer can be set by the INPUT-STRING.HEADER and INPUT-STRING.FOOTER commands, respectively. A string of characters can be given between the header and the footer, which will be sent with the formatted output (for example, [hello world], if the header is set to ’[’ and the footer to ’]’). Since the input string is saved temporarily, it appears only in the next result output. Use Setup Tool (the <Input String> option) or <ISTR> with DMCC (see SET FORMAT.TOKEN) to allow Input string in the result output.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | enable/disable

## Platforms

ALL

## Notes

Version: 5.0.0