View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How does the reader perform verification when multiple lighting configurations are enabled?

The device will start verification with the first selected lighting configuration and continue until it receives a passing overall grade. If none of the lighting configurations produce a passing grade, the image and graphics corresponding to the configuration with the best overall grade is returned to the user. The passing grade is controlled with the Minimum pass grade parameter for AIM-DPM/ISO/IEC TR 29158 and ISO 15415. The AS9132 quality metrics already produce a symbol grade that is only either a pass or fail.

Note: DM8600