View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I set with the Error LED Pulse Duration setting?

You can move the slider to the desired millisecond that is used to determine how long the Error LED pulses on fix mount devices. Error LED are found on the top of the device. Setting the slider to '0' causes the red error LED to turn off if the device log is retrieved, while every value above '0' causes the red error LED to turn off automatically after the selected time is expired.

Note: DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503