# INPUT.ACTION1

Input Line 1 Action.

Note: The given events only take effect on the bidirectional lines if you configured it in the right direction. You can change direction with the IO-LINE.DIRECTION command.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
mode | enum | [0-3] | 0: Train Code 1: Optimize Brighness 2: Set Match String 3: Optimize focus (Only for readers with a liquid lens.)
state | bool | [ON|OFF] | enable/disable

## Platforms

DM50, DM60, DM70, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM475V, DM503

## Notes

Version: 3.0.0