# HPIT.OUTPUT-CONFIG-CUSTOM-INDICATOR

Enable/Disable the use of the right HPIT indicator functionality with a given time length. As a default, none of the outputs is enabled.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
OUTPUT_NUMBER | int | [0-27] | 0 = Good read 1 = Bad read 2 = Reader programming 3 = Reader programming failure 4 = Reader programming incomplete 5 = Offline buffer low 6 = Offline buffer full 7 = Out of range 8 = Validation failure 9 = Consecutive bad read 10 = Image buffer overrun 11 = Trigger overrun 12 = Symbology learn success 13 = Symbology learn failure 14 = Train focus started 15 = Train focus success 16 = Train focus failure 17 = Optimize brightness started 18 = Optimize brightness success (Grade A) 19 = Optimize brightness success (Grade B) 20 = Optimize brightness success (Grade C) 21 = Optimize brightness failure 22 = Trigger detected 23 = Learn trigger detected 24 = Height sensor error 25 = Devlog error 26 = User event 1 27 = User event 2
state | bool | [ON|OFF] | enable/disable
TIME_LENGTH_US | int | [0 - 20000] | microseconds

## Platforms

DM370, DM380 with HPIT, DM282, DM470

## Notes

Version: 6.1.7