View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I use RTM Lean for?

Real Time Monitoring (RTM) Lean is a feature built into DataMan Setup Tool that allows for the collection and analysis of different kinds of data related to a single device on the network and its readings. The target device for this data acquisition, as well as the selection of the type of data collected, can be set up under Configuration on the ribbon menu. By default, RTM Lean collects statistical data (Read Rate, NoRead count, average decode time, trigger count, trigger overrun, buffer overflow, and process control metics, if enabled on the device).

Note: DM060,DM260,DM300,DM360,DM503, DM370, DM080, DM280, DM470,DM580, DM380, RTM_Lean