View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What settings are available under Device Time Settings?

You can select the time zone for your device from the drop-down menu. The text box below displays the the related POSIX-style time zone text of the setting, and it can be edited freely.

If Enable NTP is selected, the device synchronizes its time zone setting with the server designated in the boxes below (NTP1). The second box (NTP2) points to a second NTP server that can be used as backup, as well as to eliminate connections specific time differences between the two servers. It is sufficient to specify NTP1, but time, accuracy, and reliability increases if there are two servers involved. Note that time zone information is also used by the date object in Script-based formatting.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500