View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What are Buffered Image Settings?

Under Buffered Image Settings, you can change the size, format, and quality of the image transferred through FTP.

- size: The default image size for buffered images is the full size image. Choosing between image sizes allows the reader to perform a sub-sampling of each image, which can dramatically improve image transfer speed at the cost of some precise image details.

- format: By default, the reader stores each acquired image in a .bmp format.

- quality: Available only if you are using the .jpeg image format, this slider adjusts internal parameters that allow the reader to perform a smoothing operation on the acquired image which can reduce or enhance the transfer speed.

Note: DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500