# MIRROR.ENABLE-FOCUS-CORRECTION

Automatically adjusts focus distance between mirror movements to maintain consistent focus on a plane parallel to the HSSM front face, known as the reference plane. The current mirror position and focus is used as the reference plane when enabled.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool | [ON|OFF] | Enable/Disable focus correction between angular movements.

## Platforms

DM370, DM470 equipped with High Speed Steerable Mirror

## Notes

Version: 6.1.10