# Calibration

1. Start the DataMan Setup Tool and connect to your reader.

2. Select the Code Quality Settings task pane.

3. Check the box for Verification Enabled under the Verification tab.

4. Place the verifier against the calibration card with the symbol centered below the reader, and squeeze the trigger

5. Continue squeezing the trigger. Calibration can take several seconds

   The DataMan Setup Tool displays a graphic guide if the symbol is not precisely aligned with the reader. Adjust the position and rotation of the reader until the center of the red rectangle lies inside the green rectangle and there is no more than 10 degrees rotation between the symbol and the reader. The reader beeps once when calibration is complete.

6. The system displays a green check box that says System Calibrated under Calibration in Verification Settings.