# TRUCHECK.CALIBRATE-ON

Begins the calibration process, using a calibrated conformance standard test card. In order to calibrate successfully, RMax and RMin must match the value from the test card. The calibration symbol must be read once calibration is started.

## Actions

Command

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
RMax |  | [0.1-100.0] | The RMax value of the calibration target.
RMin |  | [0.1-100.0] | The RMSin value of the calibration target.

## Platforms

DM475V, DM8072V

## Notes

Version: 6.1.10