# REBOOT.DELAYED

Reboot the reader after delay in seconds. Rebooting the reader restores the Configuration stored in Non-Volatile Memory. Commands will not be processed for several seconds while the reader reboots.If communication settings are changed, connection with device may be lost. Note that when connected via USB-COM, the application must release the COM port.

## Actions

## Arguments

None.

## Platforms

All

## Notes

Version: 5.6.0