# IMAGEBUFFER.NO-READ-IMAGE-NUMBER

Store exactly one image.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
limit | int | [n] | In Burst trigger mode, n is the number of images in a burst
[Max Int] | In other trigger modes, there is no limit

## Platforms

DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503 only in Single, Burst, Self and Continuous modes.

## Notes

Version: 5.0.0