# HPIT.DISTANCE-BASED-TRIGGERING-ENABLED

When enabled, if the current operation mode is single (external), burst (external), or continuous (external), the HPIT ToF generates an automated trigger on signal when an object is detected inside the bounds set by the max and min distance (For more information, see: HPIT.RANGE-DETECTION-MAX-DISTANCE). The trigger automatically goes off if an out of range is detected while the trigger is ON, or if the trigger has finished its decoding task.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
enable | bool | [ON|OFF] | ON/OFF

## Platforms

DM370 with HPIT, DM380 with HPIT, DM390 with HPIT, DM470 with HPIT.

## Notes

Version: 6.1.8