# PCM.MIN-PASS

Set the overall minimum passing grade. Results under this grade will mean the reading failed.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type |  | [0-5] | 0: AIM-DPM 1: ISO-IEC 15415 2: ANSI-ISO-IEC 15416 3: SemiT10 4: 1D readability 5: DotCode Readybility
grade |  | [0-4] | 0: F 1: D 2: C 3: B 4: A

## Platforms

PCM-enabled readers

## Notes

Version: 5.7.0