# REBOOT

Reboots the reader. Rebooting the reader restores the configuration stored in non-volatile memory. Commands will not be processed for several seconds while the reader reboots. If communication settings are changed, connection with the reader may be lost.

Note: When connected through USB-COM, the application must release the COM port.

## Actions

## Arguments

None.

## Platforms

ALL

## Notes

Version: 3.0.0