# CAMERA.BURST-LENGTH

Burst length. Sets or gets the number of acquired images in Burst trigger mode.

Note: Actual maximum can be increased by reducing the camera field of view or reserving fewer images for Process Monitor/Record and Playback.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
count |  | [2-*] | number-images

## Platforms

Fixed mount readers.

## Notes

Version: 3.0.0