# System Overview

Command | Supported Platforms
--- | ---
BATTERY.CHARGE | MX-1000 and DM8000.
BATTERY.INFO | MX-1000
DATA.RESULT-TYPE | ALL
DEVICE.DESCRIPTION | ALL
DEVICE.FEATURE-KEYS | ALL
DEVICE.FIRMWARE-VER | ALL
DEVICE.NAME | ALL
DEVICE.SERIAL-NUMBER | ALL
DEVICE.TYPE | ALL
DEVICE.VARIANT | MX-1000 and MX-1502.
ERROR-LED.ON-TIME-MS | All devices with an error LED.
MOBILE-DEVICE.CHARGE-PROFILES-ENABLE | MX series
POWER.HIBERNATE-DISABLE | DM8000 wireless readers.
POWER.HIBERNATE-TIMEOUT | DM8000 wireless readers.
POWER.POWEROFF-DISABLE | DM8050, DM8600, MX-1000 and MX-1502.
POWER.POWEROFF-TIMEOUT | DM8050, DM8600, MX-1000 and MX-1502.
TUNE-BUTTON.3SEC-ACTION | DM503
TUNE-BUTTON.3SEC-ACTION | DM8600 readers
TUNE-BUTTON.SAVE-MATCH-STRING | DM503
VIBRATION.GOOD | Handheld readers, except for DM8050.