# OUTPUT.USER-CONFIGURE

Sets the beeper tone, number of beeps, LED color, and vibration state for USER_EVENT_1 or USER_EVENT_2.

Note: The DM8050 ignores the vibration state but the parameter is still required.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
event number | int | [1,2] | 1: USER_EVENT_1 2: USER_EVENT_2
beep tone | enum | [0-2] | [0]: Low [1]: Medium [2]: High
beep number | int | [0-3] | Number of beeps
LED color | enum | [0-7] | [0]: Off [1]: Blue [2]: Green [3]: Cyan [4]: Red [5]: Magenta [6]: Yellow [7]: White
vibration | bool | [ON|OFF] | ON: The reader vibrates on the given user event. OFF: The reader does not vibrate on the given user event.

## Platforms

DM8050, DM8600, DM8700, MX1000.

## Notes

Version: 5.3.0