# I2O5.CODESIZE

I2of5 Code Size. For the cmbSDK's mobile camera API, all of the Code 25 variants use the same minimum length; thus it will accept either C25.CODESIZE or I205.CODESIZE.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
any |  | [ON|OFF] | any length code
min | int | [4-max] | minimum code length
max | int | [min-80] | maximum code length

## Platforms

ALL

## Notes

Version: 3.0.0