# BLUETOOTH.HID-RECONNECT

If enabled, pulling the trigger re-establishes the Bluetooth connection to a Bluetooth Direct Connect device if the reader is paired but not connected. You can only initiate the reconnection if you enable sending HID results with the COM.USB-HID-ENABLE command.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
number | BOOL | [ON|OFF] | enable/disable

## Platforms

DM8700

## Notes

Version: 6.2.8