# LIGHT.DIRECT

Sets the quadrants on the DM70, DM150 and DM260. Possible values are ON and OFF for each segment. Example for a SET command: SET LIGHT.DIRECT ON OFF OFF ON if you want to have the top-left and bottom-right LED on.

Note: This command is deprecated. It is recommended to use LIGHT.BANKS command as an alternative with the same functionality.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
north-east | bool | [ON|OFF] | enable/disable
north-west | bool | [ON|OFF] | enable/disable
south-east | bool | [ON|OFF] | enable/disable
south-west | bool | [ON|OFF] | enable/disable

## Platforms

DM70, DM150 and DM260 readers

## Notes

Version: 5.5.0