# LIGHT.DIRECT

Sets the quadrants of the internal illumination attached to the device. Small letters refer to the inner, capital letters to the outer circle, possible values are ON and OFF for each segment. Example for a SET command: SET LIGHT.DIRECT ON OFF ON ON if you want to have the inner north, south, and west lights on.

Note: This command is deprecated. It is recommended to use LIGHT.BANKS command as an alternative with the same functionality.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
North | bool | [ON|OFF] | enable/disable
East | bool | [ON|OFF] | enable/disable
South | bool | [ON|OFF] | enable/disable
West | bool | [ON|OFF] | enable/disable

## Platforms

DM380 with HPIT

## Notes

Version: 6.5.1 SR1