# LIGHT.DIRECT

You can use the command with the DataMan verifier products that have a lighting attachment with 30, 45, and 90 degree lighting options to control the lighting panels individually. N refers to North, S to South, E to East, W to West. For example, to turn on the 90 degree light, perform: ||>SET LIGHT.DIRECT OFF OFF OFF OFF OFF OFF OFF OFF ON; To turn on the 45 degree light for all four quadrants, perform: ||SET LIGHT.DIRECT OFF OFF OFF OFF ON ON ON ON OFF

## Actions

SET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
string |  | [L1|L9] | 30N is L1 30S is L2 30E is L3 30W is L4 45N is L5 45S is L6 45E is L7 45W is L8 90 degrees is L9

## Platforms

DM8072V, DM475V

## Notes

Version: 5.7.10