# OUTPUT.RESERVED

Output Reserved for External Illumination. Line will be controlled by acquisition system when enabled.

Note: The given events only take effect on the bidirectional lines if you configured it in the right direction. You can change direction with the IO-LINE.DIRECTION command.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
line | int | [0-7] | i/o line number
reserved | bool | [ON|OFF] | enable/disable

## Platforms

Fixed mount readers, except DM50, DM60 and DM70.

## Notes

Version: 3.0.0