# WIFI.SCAN-CHANNELS

List of channels to scan on when searching for the configured SSID. Limiting the scan can improve connection and roaming performance. When you type the channel numbers in the argument, only separate them with a comma, do not use space. If you set this command to an empty string, scanning takes place on all channels. To use this command, set WIFI.BAND to 0 („Any band”).

Note: If you set WIFI.SCAN-CHANNELS to any other value than an empty string, attempts to set WIFI.BAND to anything but 0 fail with error code 104. The Regulatory Domain setting affects the availability of certain channels.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
channel_list | string | 1,2,3,4,5,6,7,8,9,10,11,12,13,36, 38,40,42,44,46,48,52,56,58, 60,64,100,104,108,112,116,120, 124,128,132,136,140,149, 153,157,161,165 | List of supported channels.

## Platforms

DM8700 Wi-Fi reader

## Notes

Version: 6.2.7