# FTP-RESULT.IP-ADDRESS

IP address of target FTP server.

Note: Uses dotted decimal form, such as "192.168.23.42".

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
string | string |  |

## Platforms

Ethernet readers and MX-1000. DM8700 base stations. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.

## Notes

Version: 3.3.0