# Mounting

The device can be mounted on a DIN rail according to EN 60715 (TS35) or screwed onto a mounting plate. Both composite and individual assembly are possible.

### Mounting Module Composites

The TBNN-S0…1TBNN-S0 is not a Cognex accessory, please contact Turck for more information. adapters can be used to build module composites for group assembly.

##### Mounting on Mounting Plate

The devices are fixed on a pre-drilled mounting plate with two M4 screws. The spacers TBNN-S0-STD2TBNN-S0-STD is not a Cognex accessory, please contact Turck for more information. are necessary for mounting module composites.

Mount the modules or the module composites according to the image below.

1. Unlock the cover flap with a flat tool (for example, a screwdriver).

2. Open the flap completely.

3. To join the DMA-EZCCM-001 module and the spacer, insert the key of the spacer into the slot of the DMA-EZCCM-001 module.

4. Flap back the cover and close it. It must engage audibly.

5. Repeat steps 1 to 4 until the module group is complete.

6. Mount the modules or the module composites according to the image below.

##### Mounting on a DIN rail (TS 35)

Single modules or module composites can be mounted on a DIN rail (TS 35) using the spacers TBNN-S0-DRS3TBNN-SO-DRS is not a Cognex accessory, please contact Turck for more information..

CAUTION: Incorrect mounting malfunction due to faulty grounding:

- Orient the spacers so that the arrow in the cover flap of every spacer points in direction to the M8 Ethernet connectors
- Connect the grounding contact of the spacer to the grounding contact of the device

1. Unlock the cover flap with a flat tool (for example, a screwdriver).

2. Open the flap completely.

3. To join the EZCCM-module and the spacer, insert the key of the spacer into the slot of the EZCCM-module (3).

4. Flap back the cover and close it. It must engage audibly.

5. Repeat steps 1 to 4 until the module group in complete.

6. Mount spacers on the right and the left side of the device.

7. Place the device or the composite on the DIN rail so that the cut-outs in the spacers enclose the DIN rail (1).

8. Close the rotating pin in the spacers by means of a screw driver.

9. Ground the device.

Note: To increase stability on the mounting rail, end brackets can be mounted on the left and right side of the modules/module composites.