# Commissioning the Device in EtherNet/IP™

Features | Description
--- | ---
Number of TCP connections | 1
Number of CIP connections | 1
Input Assembly Instance | 101
Output Assembly Instance | 110
Configuration Assembly Instance | 1

##### Adding the Prebuilt Generic Ethernet modules

Import the L5K detailed project or open the ACD sample project to find all variation of setups of daisy chain devices.

Connecting the device to the PLC:

Drop down the “Ethernet” connections in “I/O Configuration” mapping.

Drag and drop the type of configuration you need into your project.

##### Data blocks

##### Data memory Input

##### Data memory Output