# DMA-EZCCM-001 Specifications

Supply Voltage | 24 VDC
Operating temperature | -40…+70 °C
Storage temperature | -40…+85 °C
Permissible Range | 18-30 VDC Total current: maximum 4 A per voltage group Total current V1+V2: maximum 5.5 A at 70 °C per module
Operating altitude | Max. 5000 m
Protection class | IP65 IP67 IP69K
DataMan Connection | Connectors C0…C1 from V1, short-circuit proof < 55 °C: – 24 V: 1,2 A per port > 55 °C: – 24 V: 0,5 A per port
Sensor/Actuator Supply VAUX2 | Connectors C2…C3 from V2, short-circuit proof, < 55 °C: 0,14 A per port > 55 °C: 0,05 A per port
Potential isolation | Galvanic isolation of V1 and V2 voltage groups Voltage proof up to 500 VDC

System data
Transmission Ethernet | 10 Mbps 100 Mbps
Connection to Ethernet | 2 x M8, 4-pin
Protocol detection | Automatic
Web server | Default: 192.168.1.254
Service interface | Ethernet via P1 or P2

EtherNet/IP™
Address assignment | According to EtherNet/IP™ standard
Device Level Ring (DLR) | Supported
Number of TCP connections | 1
Number of CIP connections | 1
Assembly Instance | 101
Output Assembly Instance | 110
Configuration Assembly Instance | 1

PROFINET
Address assignment | DCP
Conformance class | B (RT)
MinCycleTime | 1 ms
Diagnostics | According to PROFINET Alarm Handling
Topology discovery | Supported
Media Redundancy Protocol (MRP) | Supported
Cable length | Max. 30 m

DataMan interface
Signal type | RS232
Number of channels | 2

Operation mode RS232
Signal low level | -18…-3 VDC
Signal high level | 3…18 VDC
Transmission signals | TxD, RxD
Transmission rate | 115200 bps
Transmission type | Full duplex
Cable length | 5 m at 115200 baud (max. line capacity < 2000 pF)

Digital inputs
Number of channels | 4
Connection technology inputs | M12, 5-pin
Input type | PNP
Type of input diagnostics | Channel diagnostics
Switching threshold | EN 61131-2 type 3, PNP
Signal voltage, low level | < 5 V
Signal voltage, high level | > 11 V
Low-level signal current | < 1.5 mA
High-level signal current | > 2 mA
Input delay | 0.05 ms
Electrical isolation | Galvanic isolation to P1/P2, voltage proof up to 500 VDC