# Connecting the modules to Ethernet

The DMA-EZCCM-001 module is provided with an integrated auto crossing switch with two 4-pin M8 Ethernet plug connectors for connecting to the fieldbus.

CAUTION:

Observe using the correct M8-connectors when connecting Ethernet and power cables (Ethernet: P1 and P2, power: X1and X2). Interchanging the Ethernet and the power cables can destruct the internal electronics.

Connect the device to Ethernet according to the pin assignment below.