# RecordPlayback Overview

Command | Supported Platforms
--- | ---
IMAGEBUFFER.ALLOW-OVERWRITE | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.AUTO-PREFER-CENTER | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.DELETE | DM50, DM60, DM70, DM80, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.DELETE-AFTER-TRANSFER | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.FORMAT | DM50, DM60, DM70, DM80, DM280, DM290, DM503, MX-1000, DM8000, DM300, DM360, DM370, DM390, DM470
IMAGEBUFFER.GOOD-IMAGE-MODE | DM80, DM280, DM290, DM300, DM503, DM8050, DM8600
IMAGEBUFFER.GOOD-IMAGE-RATE-BURST | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600
IMAGEBUFFER.GOOD-IMAGE-RATE-COUNT | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.GOOD-IMAGE-RATE-TIME | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.IMAGE-TYPE | DM70, DM80, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM580
IMAGEBUFFER.MAX-IMAGES-PER-RESULT | DM50, DM60, DM70, DM80, DM280, DM290,DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.MAX-NUM | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.MIN-DISTANCE | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050, DM8600.
IMAGEBUFFER.NO-READ-IMAGE-NUMBER | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503 only in Single, Burst, Self and Continuous modes.
IMAGEBUFFER.NO-READ-IMAGE-PERIOD | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, only in Single, Burst, Self and Continuous modes.
IMAGEBUFFER.NO-READ-IMAGE-RATE-BURST | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, only in Single, Burst, Self and Continuous modes.
IMAGEBUFFER.NO-READ-IMAGE-RATE-COUNT | DM80, DM280, DM290, DM503, DM300, only in Single, Burst, Self and Continuous modes.
IMAGEBUFFER.NO-READ-IMAGE-RATE-TIME | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, only in Single, Burst, Self and Continuous modes.
IMAGEBUFFER.NUM | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.OVERLAY | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
IMAGEBUFFER.QUALITY | DM50, DM60, DM70, DM80, DM280, DM290, DM503, MX-1000, DM8000, DM300, DM360, DM370, DM390, DM470
IMAGEBUFFER.RECORD | Fixed mount readers, DM8050 and DM8600.
IMAGEBUFFER.RECORD-TYPE | DM50, DM60, DM70, DM300, DM360, DM370, DM390, DM470, DM8000, DM503, MX-1000
IMAGEBUFFER.SEND-FTP | DM60, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM8000, DM503
IMAGEBUFFER.SIZE | DM50, DM60, DM70, DM80, DM280, DM290, DM503, MX-1000, DM8000, DM300, DM360, DM370, DM390, DM470
IMAGEBUFFER.SUPPRESS-IMAGES-WITH-NO-CODE | DM370, DM390, DM470
IMAGEBUFFER.TRANSFER-MODE | DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM8000, DM503, MX-1000, DM260.