# COM.RS232-INTERCHAR-DELAY

Sets or gets the internal delay between sending characters to the serial port. Only supported on DM80-USB when using the DM-RS232IO-00 cable.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
us | int | [0-5000] | milliseconds

## Platforms

DM80-USB, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM60, DM50, DM70, DM503, DM8700 RS232, DM8700 base station RS232

## Notes

Version: 5.5.0