View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Inter-message delay?

The inter-message delay, measured in milliseconds, controls the delay time between the transmission of decoded data stored in the wireless reader.

By default, the reader uses a delay of 1 millisecond, but you can increase the delay up to a maximum of 10000 milliseconds based on the needs of any application designed to accept the incoming data.

Note: DM8050, DM8070, DM8600, DM8700, MX-1000, MX-1500