View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What are Delay Mode and Code Re-Read Delay?

The Delay Mode option sets the code re-reading delay relative to either the first or the last read.

The Code Re-Read Delay (in milliseconds) option lets you specify the delay between read attempts. Specifying a non-zero value for this delay can help prevent data from overwhelming the device that is connected to your reader.

Note: DM050, DM060, DM070, DM080, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580, DM8050, DM8070, DM8600, DM8700