# Indicator LEDs

MX-1000 indicator LEDs

Type | Signal | Color | Interval | Meaning
--- | --- | --- | --- | ---
Status | Battery health | RED and GREEN | blinking | Battery health low
Configuration | GREEN | 2 short blinks/1 sec | Internal reconfiguration
Overheat protection | RED | 2 short blinks/1.5 sec | Overheat protection
Status standalone | Low battery status | RED | every 4 sec | Charged 15-10%
RED | every 2 sec | Charged 10-8%
RED | every 1 sec | Charged 8-5%
RED | every 0.5 sec | Charged < 5%
Status base station | Charging | RED | continuous | Charging
Charged | GREEN | continuous | Fully charged
Error | RED | blinking | Charging error

Charging station power LEDs

Type | Signal | Color | Interval | Meaning
--- | --- | --- | --- | ---
Status | Wireless power | RED | continuous | wireless power disconnected, there is no device in the charger bay
GREEN | continuous | wireless power connected, charging is active

Battery charger LEDs

Type | Signal | Color | Interval | Meaning
--- | --- | --- | --- | ---
Status | No battery inserted | N/A | N/A | Battery disconnected
Battery charging | RED | continuous | Charging is active
Error | RED | blinking | Charging error
Charged | GREEN | continuous | Charged