# OUTPUT.EVENTS

Output Events. Configure output line to signal based on event.

Note: The given events only take effect on the bidirectional lines if you configured it in the right direction. You can change direction with the IO-LINE.DIRECTION command.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
line | int | [0-7] | i/o line number
read | enum | [0-1] | 0: Off 1: On
no-read | enum | [0-1] | 0: Off 1: On
validation-failure | enum | [0-1] | 0: Off 1: On
trigger-overrun | enum | [0-1] | 0: Off 1: On
buffer-overflow | enum | [0-1] | 0: Off 1: On
verification-failure | enum | [0-1] | 0: Off 1: On
user event 1 | enum | [0-1] | 0: Off 1: On
user event 2 | enum | [0-1] | 0: Off 1: On

## Platforms

Fixed mount readers.

## Notes

Version: 3.0.0

Note: This is a technology preview command. It may be changed or removed in a future release.