# Decoder Overview

Command | Supported Platforms
--- | ---
AZTEC.TRAINED-MODEL | Fixed-mount readers
DATAMATRIX.DAMAGE | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470
DATAMATRIX.LEARNING-NUMROWS-NUMCOLS | DM80, DM280, DM290, DM370, DM390, DM470
DATAMATRIX.LEARNING-PARTIAL-MODEL | DM80, DM280, DM290, DM370, DM390, DM470
DATAMATRIX.LEARNING-PARTIAL-MODEL-GRIDS | Fixed mount readers
DATAMATRIX.LEARNING-VALID | DM80, DM280, DM290, DM370, DM390, DM470
DATAMATRIX.LOW-RES-2D | ALL
DATAMATRIX.PERSPECTIVE-DISTORTION | DM80, DM280, DM290, DM370, DM390, DM470
DATAMATRIX.QUALITY-METRICS | ALL
DATAMATRIX.TRAINED-MODEL | Fixed-mount readers
DECODER.1D-DATA-STITCH | DM70, DM150, DM260, DM300, DM503.
DECODER.1D-EXTENDED-RESOLUTION | DM70, DM80, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503
DECODER.1D-LEARN-ORIENT | Fixed mount readers.
DECODER.1D-QUALITY-METRICS | ALL
DECODER.1D-SHORT-QUIET-ZONE | ALL
DECODER.1D-SYMBOL-ORIENTATION | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, MX-1000, MX-1502.
DECODER.1D-USAGE | Fixed mount readers.
DECODER.AI-ENHANCER | DM290, DM390
DECODER.ALLOW-ALL-MST-RESULTS | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM70, DM150, DM260
DECODER.CENTERING-WINDOW | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470, MX-1000
DECODER.DISPLAY-TARGET | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470, MX-1000
DECODER.MAC-SCAN-TIMEOUT | DM50, DM60, DM70, DM150 DM260, DM300, DM360, DM370, DM390, DM470, MX-1000, MX1502
DECODER.REREAD-BASED-ON-SYMBOLOGY | DM370, DM390, DM470
DECODER.REREAD-MODE | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.
DECODER.REREAD-NEVER2X | ALL
DECODER.REREAD-NOT-LAST-N | All
DECODER.REREAD-TIME | ALL
DECODER.REREAD-TIME | ALL
DECODER.ROI | ALL
DECODER.TARGET-DECODING | MX-1000, MX-1502.
DECODER.TIMEOUT | Fixed mount readers.
DECODER.USE-CENTERING | DM50, DM60, DM70, DM150, DM260, DM300, DM360, DM370, DM390, DM470, MX-1000
DOTCODE.MAXIMUM-COLUMNS | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM8050X and DM8600.
DOTCODE.MAXIMUM-ROWS | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM8050X and DM8600.
DOTCODE.MINIMUM-COLUMNS | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM8050X and DM8600.
DOTCODE.MINIMUM-ROWS | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM8050X and DM8600.
DOTCODE.POLARITY | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM8050X and DM8600.
DVALID-REPORT.ENABLE | All
FILTER.IMAGE-TO-USE-SYMBOL | DM50, DM60, DM70, DM150, DM260, DM300, DM360, DM370, DM390, DM470.
FILTER.NOREAD-IMAGE | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470.
FILTER.STACK | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM390, DM470.
LIGHT.DIRECT | DM8072V, DM475V
MAXICODE.TRAINED-MODEL | Fixed-mount readers
OUTPUT.DELAY-DISTANCE | DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503.
OUTPUT.DELAY-REFERENCE | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503.
OUTPUT.DELAY-TIME | DM50, DM60, DM70, DM80, DM280, DM290, DM503, DM300, DM360, DM370, DM390, DM470.
OUTPUT.DELAY-TYPE | DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470.
OUTPUT.DELAY-TYPE | DM503
PCM-REPORT.ENABLE | All
PCM-RESULT-STRING.EXTEND | PCM-enabled readers
PCM-RESULT-STRING.METRIC-FORMAT | PCM-enabled readers
PCM-RESULT-STRING.METRIC-PREFIX | PCM-enabled readers
PCM-RESULT-STRING.METRIC-SEPARATOR | PCM-enabled readers
PCM-RESULT-STRING.OVERALL-GRADE | PCM-enabled readers
PCM-RESULT-STRING.SEPARATOR | PCM-enabled readers
PCM.CUSTOM-DESCRIPTION | PCM-enabled readers
PCM.METRIC-PARM-OVERALL | PCM-enabled readers
PCM.METRIC-PARM-REPORT | PCM-enabled readers
PCM.METRIC-PARM-THRESHOLD | PCM-enabled readers
PCM.MIN-PASS | PCM-enabled readers
PCM.USE-CUSTOM-THRESHOLDS | PCM-enabled readers
QR.DAMAGE | DM80, DM280, DM290, DM370, DM390, DM470
QR.LEARNING-GRID-SIZE | Fixed-mount readers
QR.LEARNING-PARTIAL-MODEL | Fixed-mount readers
QR.LEARNING-POLARITY | Fixed-mount readers
QR.LOW-RES-2D | ALL
QR.QUALITY-METRICS | ALL
QR.TRAINED-MODEL | Fixed-mount readers
TRUCHECK.AG | DM8072V
TRUCHECK.AG-GRADE | DM8072V
TRUCHECK.ANU | DM8072V
TRUCHECK.ANU-GRADE | DM8072V
TRUCHECK.APERTURE | DM475V, DM8072V
TRUCHECK.APERTURE-SIZE | DM475V, DM8072V
TRUCHECK.APPLICATION-CUSTOM-DATA-PARSING-STANDARD | DM475V, DM8072V
TRUCHECK.APPLICATION-CUSTOM-MAXIMUM-X-DIM | DM475V, DM8072V
TRUCHECK.APPLICATION-CUSTOM-MINIMUM-X-DIM | DM475V, DM8072V
TRUCHECK.APPLICATION-CUSTOM-PASS-GRADE | DM475V, DM8072V
TRUCHECK.APPLICATION-GS1-TABLE | DM475V, DM8072V
TRUCHECK.APPLICATION-STANDARD | DM475V, DM8072V
TRUCHECK.AUTO-BATCH | DM475V, DM8072V
TRUCHECK.BATCH-NUMBER | DM475V, DM8072V
TRUCHECK.CALIBRATE-CUSTOM-ON | DM475V, DM8072V
TRUCHECK.CALIBRATE-OFF | DM475V, DM8072V
TRUCHECK.CALIBRATE-ON | DM475V, DM8072V
TRUCHECK.CALIBRATION-DATE | DM475V, DM8072V
TRUCHECK.COMPANY-NAME | DM475V, DM8072V
TRUCHECK.CUSTOM-NOTE | DM475V, DM8072V
TRUCHECK.DECODE-GRADE | DM8072V
TRUCHECK.DOT-PEEN | DM475V, DM8072V
TRUCHECK.FPD | DM8072V
TRUCHECK.FPD-GRADE | DM8072V
TRUCHECK.GNU | DM8072V
TRUCHECK.GNU-GRADE | DM8072V
TRUCHECK.GRADING-STANDARD | DM475V, DM8072V
TRUCHECK.ISO15415-VERSION | DM280, DM290, DM370, DM380, DM470
TRUCHECK.ISO15416-VERSION | DM280, DM290, DM370, DM380, DM470
TRUCHECK.ISO29158-VERSION | DM280, DM290, DM370, DM380, DM470
TRUCHECK.METRIC-UNITS | DM475V, DM8072V
TRUCHECK.MOD-GRADE | DM8072V
TRUCHECK.OPERATOR-NAME | DM475V, DM8072V
TRUCHECK.REPORT-SECTION | DM280, DM370, DM470, DM475V, DM8072V
TRUCHECK.REPORT-SECTION-ENABLED | DM8072V
TRUCHECK.RM-GRADE | DM8072V
TRUCHECK.SC | DM8072V
TRUCHECK.SC-GRADE | DM8072V
TRUCHECK.UEC | DM8072V
TRUCHECK.UEC-GRADE | DM8072V
VERIFICATION.ENABLE | DM8072V, DM370, DM390, DM470