# IMAGEBUFFER.MAX-NUM

Maximum number of images that can be buffered.

Note: * Range varies depending depending on Camera ROI and memory allocated for burst length.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
size | int | [0-*] |

## Platforms

DM50, DM60, DM70, DM80, DM280, DM290, DM300, DM360, DM370, DM390, DM470, DM503, DM8050 and DM8600.

## Notes

Version: 4.0.0