# IO-LINE.DIRECTION

Sets the direction of the programmable I/O lines.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
line |  | [2,3] | line=2: sets direction of I/O Line 2 line=3: sets direction of I/O Line 3
direction |  | [0,1] | direction=0: defines line as output direction=1: defines line as input

## Platforms

DM280, DM290, DM360, DM370, DM390, DM470, DM580

## Notes

Version: 5.5.0