View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Industrial Protocols

EtherNet/IP protocol

To enable the reader to use the Ethernet/IP protocol, check EtherNet/IP in the Ethernet tab's Industrial Protocols box.

"The changes made require reboot to take effect." is displayed on the right side of the Communications banner. Click Save Settings and then reboot your reader.

PROFINET protocol

To enable the reader to use the PROFINET protocol, check PROFINET. You can enter the name of the station by clicking the Use Name of Station box.

"The changes made require reboot to take effect." is displayed on the right side of the Communications banner. Click Save Settings and then reboot your reader.

SLMP Protocol

To enable the reader to use the SLMP protocol, check SLMP Protocol, then set the parameters as needed.

"The changes made require reboot to take effect." is displayed on the right side of the Communications banner. Click Save Settings and then reboot the reader for the setting to take effect, either by toggling power to the reader or by scanning the Reset symbol.

Modbus TCP

To enable the reader to use the Modbus TCP protocol, check Modbus TCP, then set the parameters as needed.

"The changes made require reboot to take effect." is displayed on the right side of the Communications banner. Click Save Settings and then reboot the reader for the setting to take effect, either by toggling power to the reader or by scanning the Reset symbol.

EtherCAT

EtherCAT is the default protocol of the DM280 EtherCAT reader. To switch to another protocol, uncheck EtherCAT.

"The changes made require reboot to take effect." is displayed on the right side of the Communications banner. Click Save Settings and then reboot the reader for the setting to take effect, either by toggling power to the reader or by scanning the Reset symbol.

EtherNet/IP, PROFINET, SLMP Protocol, Modbus TCP, or EtherCAT selection grayed out

Only one Ethernet industrial protocol may be used at a given time. When one protocol is selected, the other is unavailable.

Note: DM060, DM070, DM080, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM470, DM503, DM580, DM8050, DM8070, DM8600, DM8700, DM8700Base, DM8000Base