View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 290

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 390

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How does data formatting work?

On the Basic pane you can select what type of formatting you want to use.

You use the Standard pane to construct a customized output string using pre-defined building blocks on the individual symbology tabs:

- The output string starts with whatever text you enter in the Leading Text field.

- Select items from the lists in the General, Validation, and (when applicable, to the) Metrics tabs, and click Add to add them to the output string. To add a specific range of characters from the decoded data, click Set sub-string range, then enter the range of characters to add (such as 1-3,5,8,10-), then click on Sub-string in the list and click the Add button.

- The output string also includes any text that you add to the Terminating Text field.

- To terminate the entire string with a carriage return/line feed pair, check the CR/LF checkbox.

Note: default, DMAE50, DM050, DM060, DM070, DM080, DM150, DM260, DM280, DM290, DM300, DM360, DM370, DM380, DM390, DM380, DM390, DM470, DM503, DM580, DM7500, DM8050, DM8070, DM8600, DM8700, MX-1000, MX-1500